**Conference for Food Protection**

**2016 Issue Form**

**Issue: 2016 I-043**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Council Recommendation:** | Accepted asSubmitted |  | Accepted as Amended |  | No Action |  |
| **Delegate Action:** | Accepted |  | Rejected |  |  |  |

*All information above the line is for conference use only.*

**Title:**

Harmonizing Direct Drain Connection Allowances with Plumbing Codes

**Recommended Solution: The Conference recommends...:**

a letter be sent to the FDA requesting the 2013 Food Code be amended as follows (language to be added is underlined):

**Paragraph 5-402.11(C)**

(C) If allowed by LAW, a WAREWASHING machine or WAREWASHING sink may have a direct connection between its waste outlet and a floor drain when the machine or sink is located within 1.5 m (5 feet) of a trapped floor drain and the machine or sink outlet is connected to the inlet side of a properly vented floor drain trap.

It is the policy of the Conference for Food Protection to not accept Issues that would endorse a brand name or a commercial proprietary process.