**Conference for Food Protection**

**2018 Issue Form**

**Issue: 2018 I-008**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Council Recommendation:** | Accepted asSubmitted |  | Accepted as Amended |  | No Action |  |
| **Delegate Action:** | Accepted |  | Rejected |  |  |  |

*All information above the line is for conference use only.*

**Title:**

Amend Food Code - Backflow Prevention, 5-402.11

**Recommended Solution: The Conference recommends...:**

that a letter be sent to the FDA requesting that section 5-402.11 of the most current edition of the Food Code be amended as follows (new language is underlined; language to be deleted is in strikethrough format):

(A) Except as specified in (B) (C) and (D), a direct connection may not exist between the sewage system and a drain originating from EQUIPMENT in which FOOD, portable EQUIPMENT, or UTENSILS are placedP...

...~~(C)~~(D) ~~If allowed by LAW~~, A ~~a~~ WAREWASHING machine may have a direct connection between its waste outlet and a floor drain when the machine is located within 1.5 m (5 feet) of a trapped floor drain and the machine outlet is connected to the inlet side of a properly vented floor drain trap.

~~(D) If allowed by LAW,~~ A ~~a~~ WAREWASHING or culinary sink may have a direct connection.

It is the policy of the Conference for Food Protection to not accept Issues that would endorse a brand name or a commercial proprietary process.